    001    //$HeadURL: https://svn.wald.intevation.org/svn/deegree/base/branches/2.4_testing/src/org/deegree/ogcwebservices/sos/configuration/SensorConfiguration.java $
    002    /*----------------------------------------------------------------------------
    003     This file is part of deegree, http://deegree.org/
    004     Copyright (C) 2001-2009 by:
    005       Department of Geography, University of Bonn
    006     and
    007       lat/lon GmbH
    008
    009     This library is free software; you can redistribute it and/or modify it under
    010     the terms of the GNU Lesser General Public License as published by the Free
    011     Software Foundation; either version 2.1 of the License, or (at your option)
    012     any later version.
    013     This library is distributed in the hope that it will be useful, but WITHOUT
    014     ANY WARRANTY; without even the implied warranty of MERCHANTABILITY or FITNESS
    015     FOR A PARTICULAR PURPOSE. See the GNU Lesser General Public License for more
    016     details.
    017     You should have received a copy of the GNU Lesser General Public License
    018     along with this library; if not, write to the Free Software Foundation, Inc.,
    019     59 Temple Place, Suite 330, Boston, MA 02111-1307 USA
    020
    021     Contact information:
    022
    023     lat/lon GmbH
    024     Aennchenstr. 19, 53177 Bonn
    025     Germany
    026     http://lat-lon.de/
    027
    028     Department of Geography, University of Bonn
    029     Prof. Dr. Klaus Greve
    030     Postfach 1147, 53001 Bonn
    031     Germany
    032     http://www.geographie.uni-bonn.de/deegree/
    033
    034     e-mail: info@deegree.org
    035    ----------------------------------------------------------------------------*/
    036    package org.deegree.ogcwebservices.sos.configuration;
    037
    038    import java.util.ArrayList;
    039
    040    /**
    041     * represents a sensor configuration
    042     *
    043     * @author <a href="mailto:mkulbe@lat-lon.de">Matthias Kulbe </a>
    044     * @author last edited by: $Author:wanhoff$
    045     *
    046     * @version $Revision: 23585 $, $Date:20.03.2007$
    047     */
    048    public class SensorConfiguration {
    049
    050        private String id = null;
    051
    052        private String idPropertyValue = null;
    053
    054        private String sourceServerId = null;
    055
    056        private ArrayList<MeasurementConfiguration> measurementConfigurations = new ArrayList<MeasurementConfiguration>();
    057
    058        /**
    059         * constructor
    060         *
    061         * @param id
    062         * @param idPropertyValue
    063         * @param sourceServerId
    064         * @param measurements
    065         */
    066        public SensorConfiguration( String id, String idPropertyValue, String sourceServerId,
    067                                    MeasurementConfiguration[] measurements ) {
    068            this.id = id;
    069            this.idPropertyValue = idPropertyValue;
    070            this.sourceServerId = sourceServerId;
    071
    072            if ( measurements != null ) {
    073                for ( int i = 0; i < measurements.length; i++ ) {
    074                    this.measurementConfigurations.add( measurements[i] );
    075                }
    076            } else {
    077                // it's a TODO
    078            }
    079        }
    080
    081        /**
    082         * returns all measurements
    083         *
    084         * @return all measurements
    085         */
    086        public MeasurementConfiguration[] getMeasurementConfigurations() {
    087            return measurementConfigurations.toArray( new MeasurementConfiguration[measurementConfigurations.size()] );
    088        }
    089
    090        /**
    091         * returns the first measurement; is the default if the user don't request a special measurement
    092         *
    093         * @return the first measurement
    094         */
    095        public MeasurementConfiguration getFirstMeasurementConfiguration() {
    096            return this.measurementConfigurations.get( 0 );
    097        }
    098
    099        /**
    100         *
    101         * @return id
    102         */
    103        public String getId() {
    104            return id;
    105        }
    106
    107        /**
    108         *
    109         * @return idPropertyValue
    110         */
    111        public String getIdPropertyValue() {
    112            return idPropertyValue;
    113        }
    114
    115        /**
    116         *
    117         * @return sourceServerId
    118         */
    119        public String getSourceServerId() {
    120            return sourceServerId;
    121        }
    122
    123        @Override
    124        public boolean equals( Object obj ) {
    125            if ( !( obj instanceof SensorConfiguration ) ) {
    126                return false;
    127            }
    128            if ( this.getId().equals( ( (SensorConfiguration) obj ).getId() ) ) {
    129                return true;
    130            }
    131            return false;
    132        }
    133
    134        /**
    135         * returns the Measurement Config by the given id
    136         *
    137         * @param id
    138         * @return the Measurement Config by the given id
    139         */
    140        public MeasurementConfiguration getMeasurementById( String id ) {
    141            for ( int i = 0; i < this.measurementConfigurations.size(); i++ ) {
    142                if ( this.measurementConfigurations.get( i ).getId().equals( id ) ) {
    143                    return this.measurementConfigurations.get( i );
    144                }
    145            }
    146            return null;
    147        }
    148
    149    }