    001    //$HeadURL: $
    002    /*----------------------------------------------------------------------------
    003     This file is part of deegree, http://deegree.org/
    004     Copyright (C) 2001-2009 by:
    005       Department of Geography, University of Bonn
    006     and
    007       lat/lon GmbH
    008
    009     This library is free software; you can redistribute it and/or modify it under
    010     the terms of the GNU Lesser General Public License as published by the Free
    011     Software Foundation; either version 2.1 of the License, or (at your option)
    012     any later version.
    013     This library is distributed in the hope that it will be useful, but WITHOUT
    014     ANY WARRANTY; without even the implied warranty of MERCHANTABILITY or FITNESS
    015     FOR A PARTICULAR PURPOSE. See the GNU Lesser General Public License for more
    016     details.
    017     You should have received a copy of the GNU Lesser General Public License
    018     along with this library; if not, write to the Free Software Foundation, Inc.,
    019     59 Temple Place, Suite 330, Boston, MA 02111-1307 USA
    020
    021     Contact information:
    022
    023     lat/lon GmbH
    024     Aennchenstr. 19, 53177 Bonn
    025     Germany
    026     http://lat-lon.de/
    027
    028     Department of Geography, University of Bonn
    029     Prof. Dr. Klaus Greve
    030     Postfach 1147, 53001 Bonn
    031     Germany
    032     http://www.geographie.uni-bonn.de/deegree/
    033
    034     e-mail: info@deegree.org
    035    ----------------------------------------------------------------------------*/
    036
    037    package org.deegree.ogcwebservices.wcts.operation;
    038
    039    import org.deegree.i18n.Messages;
    040    import org.deegree.model.crs.CoordinateSystem;
    041    import org.deegree.ogcwebservices.wcts.data.TransformableData;
    042    import org.deegree.owscommon_1_1_0.Manifest;
    043
    044    /**
    045     * <code>TransformResponse</code> wraps the requested inputdata (e.g. the metadata) and the transformed feature
    046     * collections.
    047     *
    048     * @author <a href="mailto:bezema@lat-lon.de">Rutger Bezema</a>
    049     *
    050     * @author last edited by: $Author:$
    051     *
    052     * @version $Revision:$, $Date:$
    053     *
    054     */
    055    public class TransformResponse {
    056
    057        private final boolean store;
    058
    059        private final Manifest inputData;
    060
    061        private final TransformableData<?> transformableData;
    062
    063        private final int dataPresentation;
    064
    065        private final CoordinateSystem sourceCRS;
    066
    067        private final CoordinateSystem targetCRS;
    068
    069        /**
    070         * @param sourceCRS
    071         *            defining the source crs of the transformable data.
    072         * @param targetCRS
    073         *            defining the target crs of the transformable data.
    074         * @param dataPresentation
    075         *            a flag signaling the way the data was presented to the wcts. Valid values are {@link Transform#INLINE}
    076         *            and {@link Transform#MULTIPART}. If another value is given, {@link Transform#MULTIPART} is assumed.
    077         * @param store
    078         *            true if the transformableData should be stored, false otherwise.
    079         *
    080         * @param inputData
    081         *            may be <code>null</code>. Meaning the request did not provide any inputdata or it was a kvp
    082         *            request.
    083         * @param transformableData
    084         *            the transformed data.
    085         * @throws IllegalArgumentException
    086         *             if the transformableData object is <code>null</code>.
    087         */
    088        public TransformResponse( CoordinateSystem sourceCRS, CoordinateSystem targetCRS, int dataPresentation,
    089                                  boolean store, Manifest inputData, TransformableData<?> transformableData )
    090                                throws IllegalArgumentException {
    091            this.sourceCRS = sourceCRS;
    092            this.targetCRS = targetCRS;
    093            if ( dataPresentation != Transform.INLINE && dataPresentation != Transform.MULTIPART ) {
    094                dataPresentation = Transform.MULTIPART;
    095            }
    096            this.dataPresentation = dataPresentation;
    097            this.store = store;
    098            this.inputData = inputData;
    099            if ( transformableData == null ) {
    100                throw new IllegalArgumentException( Messages.getMessage( "WCTS_MISSING_ARGUMENT", transformableData ) );
    101            }
    102            this.transformableData = transformableData;
    103        }
    104
    105        /**
    106         * @return true if the data should be stored.
    107         */
    108        public final boolean shouldStore() {
    109            return store;
    110        }
    111
    112        /**
    113         * @return the inputData, may be <code>null</code>
    114         */
    115        public final Manifest getInputData() {
    116            return inputData;
    117        }
    118
    119        /**
    120         * @return the transformableData, will never be <code>null</code>
    121         */
    122        public final TransformableData<?> getTransformableData() {
    123            return transformableData;
    124        }
    125
    126        /**
    127         * @return a flag signaling the way the data was presented to the wcts. Valid values are {@link Transform#INLINE}
    128         *         and {@link Transform#MULTIPART}.
    129         */
    130        public final int getDataPresentation() {
    131            return dataPresentation;
    132        }
    133
    134        /**
    135         * @return the sourceCRS
    136         */
    137        public final CoordinateSystem getSourceCRS() {
    138            return sourceCRS;
    139        }
    140
    141        /**
    142         * @return the targetCRS
    143         */
    144        public final CoordinateSystem getTargetCRS() {
    145            return targetCRS;
    146        }
    147
    148    }